| **NAME** | **COMPANY / ORGANISATION** | **DATE** | **ASBESTOS CONTAINING MATERIAL RELATED WORK UNDERTAKEN*****(Include any assessment concerning asbestos that took place before the work was carried out)*** | **REFERENCE*****(Include sample numbers, report numbers, quote number and/or purchase order number etc.)*** | **COMMENTS / STATUS** |
| --- | --- | --- | --- | --- | --- |
| *xxx* | *SLR Consulting Australia Pty Ltd* | *20-21 May 2013* | *Asbestos Building Materials Survey* | *Report No 620.10797.00000/01/ASR* | *Sample numbers noted in Register*  |
|  | *Insert Company who did work* | *February 2014* | *Black Electrical Backing Board (BEBB) in Switchboard, Southern side, within fuse box to the wall*  |  *Insert job/purchase order reference* | *Assumed ACM Removed (BEBB)**New switchboard installed* |
|  | *Insert Company who did work* |  | *Building 1, Lower Ground Level, FCS Ceiling in Bathroom adjacent to rental offices area - above shower and wash basin ONLY had drop ceiling installed* | *Insert job/purchase order reference* | *Assumed ACM remains in situ behind drop ceiling which was installed above shower and wash basin area only* |
|  | *Insert Company who did work* | *September 2014* | *Main Worship Centre, Lower Ground, Exterior Eastern aspect -ACM Steps removed and replaced* | ***Sample no 620.10797.S10****; Insert job/purchase order reference* | *ACM steps removed and replaced with nonhazardous materials* |
| *xxx,*  | *Uniting Church xx Location and xx position* | *25 July 2018* | *Physical inspection of ACM in situ as identified in the ACM Register*  | *As per existing ACM Register* | *All ACM inspected, in good condition and stable - except as below* |
| *Vestry Room - Minor hairline crack in ceiling tile – intact* | *As per existing ACM Register* | *To seal with waterproof sealant e.g. Emer-Coat Clear Sealer and Emer-clad paint*  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |
|  |  |  |  |  |  |